Circuit ALU2 routed on X4000-type FPGA with F_s = 3, channel width W = 9, and F_c = W , using the IKMB routing algorithm.

Complete information is available on the World Wide Web at URL http://www.cs.virginia.edu/~robins/.